3 phase with secondary underbuild

Insulated wire